Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 09 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 0D 00 00 00
#
name: I
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 0F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 10 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 11 00 00 00
#
name: CHANNEL_+
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 20 00 00 00
#
name: CHANNEL_-
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 21 00 00 00
#
name: AV
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 38 00 00 00
#
name: SETUP
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 54 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 58 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 59 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 5A 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 5B 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 5C 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 6D 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 6E 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 6F 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 70 00 00 00
#
name: HELP
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 81 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 83 00 00 00
#
name: FOXTEL
type: parsed
protocol: NECext
address: 21 A0 00 00
command: 8E 00 00 00
#
name: TV_GUIDE
type: parsed
protocol: NECext
address: 21 A0 00 00
command: CC 00 00 00
#
name: BOX_OFFICE
type: parsed
protocol: NECext
address: 21 A0 00 00
command: D5 00 00 00
#
name: PLANNER
type: parsed
protocol: NECext
address: 21 A0 00 00
command: F4 00 00 00
#
name: ACTIVE
type: parsed
protocol: NECext
address: 21 A0 00 00
command: FD 00 00 00
