Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 01 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 01 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 01 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 01 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 01 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 01 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 01 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 01 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 01 00 00 00
command: 09 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0A 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 11 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 12 00 00 00
#
name: AB
type: parsed
protocol: NECext
address: 01 00 00 00
command: 13 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 01 00 00 00
command: 14 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 01 00 00 00
command: 15 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 01 00 00 00
command: 16 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 17 00 00 00
#
name: VTMix
type: parsed
protocol: NECext
address: 01 00 00 00
command: 18 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 01 00 00 00
command: 18 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 01 00 00 00
command: 1B 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 24 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 25 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 29 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 01 00 00 00
command: 2A 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 01 00 00 00
command: 30 00 00 00
#
name: Break
type: parsed
protocol: NECext
address: 01 00 00 00
command: 30 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 01 00 00 00
command: 32 00 00 00
#
name: VTOff
type: parsed
protocol: NECext
address: 01 00 00 00
command: 32 00 00 00
#
name: VTStop
type: parsed
protocol: NECext
address: 01 00 00 00
command: 33 00 00 00
#
name: VTOn
type: parsed
protocol: NECext
address: 01 00 00 00
command: 34 00 00 00
#
name: 102ND
type: parsed
protocol: NECext
address: 01 00 00 00
command: 3C 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 01 00 00 00
command: 48 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 01 00 00 00
command: 49 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 01 00 00 00
command: 4A 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 01 00 00 00
command: 4B 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 01 00 00 00
command: 5F 00 00 00
