Filetype: IR signals file
Version: 1
# 
# TILVIEW DVB-T
#
name: Power
type: parsed
protocol: NEC
address: 35 00 00 00
command: 01 00 00 00
# 
name: TV/RADIO
type: parsed
protocol: NEC
address: 35 00 00 00
command: 18 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 35 00 00 00
command: 12 00 00 00
# 
name: VOL -
type: parsed
protocol: NEC
address: 35 00 00 00
command: 00 00 00 00
# 
name: VOL +
type: parsed
protocol: NEC
address: 35 00 00 00
command: 07 00 00 00
# 
name: REPEAT
type: parsed
protocol: NEC
address: 35 00 00 00
command: 06 00 00 00
# 
name: CH -
type: parsed
protocol: NEC
address: 35 00 00 00
command: 04 00 00 00
# 
name: CH +
type: parsed
protocol: NEC
address: 35 00 00 00
command: 0B 00 00 00
# 
name: GOTO
type: parsed
protocol: NEC
address: 35 00 00 00
command: 0A 00 00 00
# 
name: BACKWARD
type: parsed
protocol: NEC
address: 35 00 00 00
command: 08 00 00 00
# 
name: SKIP BACKBARDS
type: parsed
protocol: NEC
address: 35 00 00 00
command: 0F 00 00 00
# 
name: FAV
type: parsed
protocol: NEC
address: 35 00 00 00
command: 0E 00 00 00
# 
name: FORWARD
type: parsed
protocol: NEC
address: 35 00 00 00
command: 43 00 00 00
# 
name: SKIP FORWARD
type: parsed
protocol: NEC
address: 35 00 00 00
command: 13 00 00 00
# 
name: AUDIO
type: parsed
protocol: NEC
address: 35 00 00 00
command: 09 00 00 00
# 
name: MENU
type: parsed
protocol: NEC
address: 35 00 00 00
command: 5B 00 00 00
# 
name: INFO
type: parsed
protocol: NEC
address: 35 00 00 00
command: 5A 00 00 00
# 
name: EPG
type: parsed
protocol: NEC
address: 35 00 00 00
command: 4E 00 00 00
# 
name: EXIT
type: parsed
protocol: NEC
address: 35 00 00 00
command: 16 00 00 00
# 
name: OK
type: parsed
protocol: NEC
address: 35 00 00 00
command: 15 00 00 00
# 
name: UP
type: parsed
protocol: NEC
address: 35 00 00 00
command: 17 00 00 00
# 
name: RIGHT
type: parsed
protocol: NEC
address: 35 00 00 00
command: 41 00 00 00
# 
name: DOWN
type: parsed
protocol: NEC
address: 35 00 00 00
command: 1A 00 00 00
# 
name: LEFT
type: parsed
protocol: NEC
address: 35 00 00 00
command: 42 00 00 00
# 
name: P -
type: parsed
protocol: NEC
address: 35 00 00 00
command: 0D 00 00 00
# 
name: LIST
type: parsed
protocol: NEC
address: 35 00 00 00
command: 14 00 00 00
# 
name: RECALL
type: parsed
protocol: NEC
address: 35 00 00 00
command: 1E 00 00 00
# 
name: P +
type: parsed
protocol: NEC
address: 35 00 00 00
command: 40 00 00 00
# 
name: RED
type: parsed
protocol: NEC
address: 35 00 00 00
command: 51 00 00 00
# 
name: GREEN
type: parsed
protocol: NEC
address: 35 00 00 00
command: 52 00 00 00
# 
name: YELLOW
type: parsed
protocol: NEC
address: 35 00 00 00
command: 53 00 00 00
# 
name: BLUE
type: parsed
protocol: NEC
address: 35 00 00 00
command: 54 00 00 00
# 
name: REC
type: parsed
protocol: NEC
address: 35 00 00 00
command: 55 00 00 00
# 
name: PLAY
type: parsed
protocol: NEC
address: 35 00 00 00
command: 56 00 00 00
# 
name: PAUSE
type: parsed
protocol: NEC
address: 35 00 00 00
command: 57 00 00 00
# 
name: STOP
type: parsed
protocol: NEC
address: 35 00 00 00
command: 10 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 35 00 00 00
command: 49 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 35 00 00 00
command: 4A 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 35 00 00 00
command: 4B 00 00 00
# 
name: TTX
type: parsed
protocol: NEC
address: 35 00 00 00
command: 5E 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 35 00 00 00
command: 45 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 35 00 00 00
command: 46 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 35 00 00 00
command: 47 00 00 00
# 
name: SUBTITLE
type: parsed
protocol: NEC
address: 35 00 00 00
command: 5F 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 35 00 00 00
command: 58 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 35 00 00 00
command: 59 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 35 00 00 00
command: 5C 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 35 00 00 00
command: 5D 00 00 00
