Filetype: IR signals file
Version: 1
#
name: VIEW
type: parsed
protocol: NECext
address: 18 00 00 00
command: 16 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 18 00 00 00
command: 19 00 00 00
#
name: RECALL
type: parsed
protocol: NECext
address: 18 00 00 00
command: 1B 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 18 00 00 00
command: 1D 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 18 00 00 00
command: 2C 00 00 00
