Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: NECext
address: EA C7 00 00
command: 17 E8 00 00
# 
name: Home
type: parsed
protocol: NECext
address: EA C7 00 00
command: 03 FC 00 00
# 
name: Left
type: parsed
protocol: NECext
address: EA C7 00 00
command: 1E E1 00 00
# 
name: Select
type: parsed
protocol: NECext
address: EA C7 00 00
command: 2A D5 00 00
# 
name: Right
type: parsed
protocol: NECext
address: EA C7 00 00
command: 2D D2 00 00
# 
name: MUTE
type: parsed
protocol: NECext
address: EA C7 00 00
command: 20 DF 00 00
# 
name: VOL+
type: parsed
protocol: NECext
address: EA C7 00 00
command: 0F F0 00 00
# 
name: VOL-
type: parsed
protocol: NECext
address: EA C7 00 00
command: 10 EF 00 00
