Filetype: IR signals file
Version: 1
#
name: OFF
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 01 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 02 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 03 00 00 00
#
name: IN_1
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 05 00 00 00
#
name: IN_3
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 06 00 00 00
#
name: IN_8
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 07 00 00 00
#
name: IN_2
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 09 00 00 00
#
name: IN_7
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 0B 00 00 00
#
name: IN_4
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 0D 00 00 00
#
name: IN_5
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 0F 00 00 00
#
name: STA_-
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 17 00 00 00
#
name: STA_+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 18 00 00 00
#
name: TUN_-
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 1B 00 00 00
#
name: TUN_+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 1C 00 00 00
#
name: CUR_LEFT
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 1F 00 00 00
#
name: CUR_RIGHT
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 20 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 23 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 24 00 00 00
#
name: +10
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 29 00 00 00
#
name: CUR_DOWN
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 2D 00 00 00
#
name: CUR_UP
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 2E 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 2F 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 30 00 00 00
#
name: SEL/ENTER
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 30 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 31 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 32 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 33 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 35 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 36 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 37 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 39 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 3A 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 3B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 3E 00 00 00
#
name: ZONE
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 3F 00 00 00
#
name: SAVE
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 40 00 00 00
#
name: IN_6
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 4A 00 00 00
#
name: PRESET_+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 4B 00 00 00
#
name: D-IN
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 5A 00 00 00
#
name: BASS_-
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 65 00 00 00
#
name: SOURCE_+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 66 00 00 00
#
name: IN_9
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 6E 00 00 00
#
name: AM
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 76 00 00 00
#
name: TREBLE_-
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 79 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 7D 00 00 00
#
name: FM
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: 8E 00 00 00
#
name: POWER_ON/OFF
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: A2 00 00 00
#
name: SOURCE_-
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: A6 00 00 00
#
name: PRESET_-
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: C6 00 00 00
#
name: LOUDNESS
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: CF 00 00 00
#
name: BASS_+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: E5 00 00 00
#
name: M
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: EB 00 00 00
#
name: TREBLE_+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: F9 00 00 00
#
name: V+
type: parsed
protocol: NECext
address: 2B 4D 00 00
command: FA 00 00 00
