Filetype: IR signals file
Version: 1
#
name: DISC
type: parsed
protocol: NECext
address: B8 00 00 00
command: 08 00 00 00
#
name: BAND___TUNER
type: parsed
protocol: NECext
address: B8 00 00 00
command: 8F 00 00 00
#
name: PHONO
type: parsed
protocol: NECext
address: B8 00 00 00
command: 90 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: B8 00 00 00
command: 91 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: B8 00 00 00
command: 92 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: B8 00 00 00
command: 93 00 00 00
#
name: TAPE_1
type: parsed
protocol: NECext
address: B8 00 00 00
command: 94 00 00 00
#
name: TAPE_2_(_MONITOR_)
type: parsed
protocol: NECext
address: B8 00 00 00
command: 95 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: B8 00 00 00
command: 96 00 00 00
#
name: P.CALL
type: parsed
protocol: NECext
address: B8 00 00 00
command: 99 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9A 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9D 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: B8 00 00 00
command: C9 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: CB 00 00 00
#
name: SKIP_REV
type: parsed
protocol: NECext
address: B8 00 00 00
command: CE 00 00 00
#
name: SKIP_FWD
type: parsed
protocol: NECext
address: B8 00 00 00
command: CF 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D0 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D1 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: B8 00 00 00
command: D2 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: B8 00 00 00
command: D3 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: B8 00 00 00
command: D5 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D8 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D9 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: B8 00 00 00
command: DA 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: B8 00 00 00
command: DB 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: B8 00 00 00
command: DD 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: B8 00 00 00
command: DE 00 00 00
