Filetype: IR signals file
Version: 1
#
# HUMAX RM-F04
# Autogenerated from ircodes/HUMAX/RM-F04.xml
#
name: POWER
type: parsed
protocol: NECext
address: 08 00 00 00
command: FF 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 08 00 00 00
command: E7 18 00 00
#
name: 1
type: parsed
protocol: NECext
address: 08 00 00 00
command: 3F C0 00 00
#
name: 2
type: parsed
protocol: NECext
address: 08 00 00 00
command: DF 20 00 00
#
name: 3
type: parsed
protocol: NECext
address: 08 00 00 00
command: 5F A0 00 00
#
name: 4
type: parsed
protocol: NECext
address: 08 00 00 00
command: 9F 60 00 00
#
name: 5
type: parsed
protocol: NECext
address: 08 00 00 00
command: 1F E0 00 00
#
name: 6
type: parsed
protocol: NECext
address: 08 00 00 00
command: EF 10 00 00
#
name: 7
type: parsed
protocol: NECext
address: 08 00 00 00
command: 6F 90 00 00
#
name: 8
type: parsed
protocol: NECext
address: 08 00 00 00
command: AF 50 00 00
#
name: 9
type: parsed
protocol: NECext
address: 08 00 00 00
command: 2F D0 00 00
#
name: TV PORTAL
type: parsed
protocol: NECext
address: 08 00 00 00
command: 2D D2 00 00
#
name: 0
type: parsed
protocol: NECext
address: 08 00 00 00
command: CF 30 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 08 00 00 00
command: 8F 70 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 08 00 00 00
command: F9 06 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 08 00 00 00
command: B9 46 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 08 00 00 00
command: 39 C6 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 08 00 00 00
command: 79 86 00 00
#
name: REV
type: parsed
protocol: NECext
address: 08 00 00 00
command: 59 A6 00 00
#
name: FWD
type: parsed
protocol: NECext
address: 08 00 00 00
command: D9 26 00 00
#
name: PREV
type: parsed
protocol: NECext
address: 08 00 00 00
command: 99 66 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 08 00 00 00
command: 19 E6 00 00
#
name: R
type: parsed
protocol: NECext
address: 08 00 00 00
command: C7 38 00 00
#
name: G
type: parsed
protocol: NECext
address: 08 00 00 00
command: 47 B8 00 00
#
name: Y
type: parsed
protocol: NECext
address: 08 00 00 00
command: A7 58 00 00
#
name: B
type: parsed
protocol: NECext
address: 08 00 00 00
command: 87 78 00 00
#
name: MEDIA
type: parsed
protocol: NECext
address: 08 00 00 00
command: 09 F6 00 00
#
name: UP
type: parsed
protocol: NECext
address: 08 00 00 00
command: 77 88 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 27 D8 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 08 00 00 00
command: B7 48 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 08 00 00 00
command: 37 C8 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 08 00 00 00
command: D7 28 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 08 00 00 00
command: 97 68 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 08 00 00 00
command: 57 A8 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 08 00 00 00
command: 7D 82 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 08 00 00 00
command: 07 F8 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 08 00 00 00
command: 4D B2 00 00
#
name: CH/PAGE+
type: parsed
protocol: NECext
address: 08 00 00 00
command: F7 08 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 08 00 00 00
command: FD 02 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 08 00 00 00
command: 3D C2 00 00
#
name: CH/PAGE-
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0F F0 00 00
#
name: OPTION
type: parsed
protocol: NECext
address: 08 00 00 00
command: BD 42 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 08 00 00 00
command: 5D A2 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 9D 62 00 00
#
name: TV/RADIO
type: parsed
protocol: NECext
address: 08 00 00 00
command: 4F B0 00 00
#
name: TELETEXT
type: parsed
protocol: NECext
address: 08 00 00 00
command: 89 76 00 00
#
name: FAV +
type: parsed
protocol: NECext
address: 08 00 00 00
command: A9 56 00 00
#
name: FAV LIST
type: parsed
protocol: NECext
address: 08 00 00 00
command: 29 D6 00 00
#
name: SLOW FWD
type: parsed
protocol: NECext
address: 08 00 00 00
command: C9 36 00 00
#
name: SOURCE
type: parsed
protocol: NECext
address: 08 00 00 00
command: BF 40 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 08 00 00 00
command: CD 32 00 00
#
name: V FORMAT
type: parsed
protocol: NECext
address: 08 00 00 00
command: 0D F2 00 00
#
name: WIDE
type: parsed
protocol: NECext
address: 08 00 00 00
command: 8D 72 00 00
