Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 09 00 00 00
#
name: 102ND
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 0A 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 10 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 11 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 15 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 18 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 19 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1A 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1B 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1C 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 1D 00 00 00
#
name: search_left
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 28 00 00 00
#
name: search_right
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 29 00 00 00
#
name: tv/vtr
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 2A 00 00 00
#
name: still
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 31 00 00 00
#
name: fine_up
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 44 00 00 00
#
name: fine_down
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 45 00 00 00
#
name: counter_reset
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 46 00 00 00
#
name: goto
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 4C 00 00 00
#
name: input_sel
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 4F 00 00 00
#
name: exe
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 51 00 00 00
#
name: quick_timer
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 52 00 00 00
#
name: timer_next
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 61 00 00 00
#
name: timer_clear
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 63 00 00 00
#
name: timer_check
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 64 00 00 00
#
name: timer_rec
type: parsed
protocol: NECext
address: 0B 00 00 00
command: 65 00 00 00
