Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: A8 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: A8 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A8 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A8 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A8 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A8 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A8 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A8 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A8 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A8 00 00 00
command: 09 00 00 00
#
name: D/A.CX
type: parsed
protocol: NECext
address: A8 00 00 00
command: 0C 00 00 00
#
name: SCAN_>>
type: parsed
protocol: NECext
address: A8 00 00 00
command: 10 00 00 00
#
name: SCAN_<<
type: parsed
protocol: NECext
address: A8 00 00 00
command: 11 00 00 00
#
name: CHAPTER/FRAME_TIME
type: parsed
protocol: NECext
address: A8 00 00 00
command: 13 00 00 00
#
name: STOP/EJECT_[]
type: parsed
protocol: NECext
address: A8 00 00 00
command: 16 00 00 00
#
name: PLAY_>
type: parsed
protocol: NECext
address: A8 00 00 00
command: 17 00 00 00
#
name: PAUSE_
type: parsed
protocol: NECext
address: A8 00 00 00
command: 18 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A8 00 00 00
command: 1C 00 00 00
#
name: EDIT
type: parsed
protocol: NECext
address: A8 00 00 00
command: 1D 00 00 00
#
name: AUDIO_MONITOR
type: parsed
protocol: NECext
address: A8 00 00 00
command: 1E 00 00 00
#
name: +10
type: parsed
protocol: NECext
address: A8 00 00 00
command: 1F 00 00 00
#
name: JOG_FORWARD_+
type: parsed
protocol: NECext
address: A8 00 00 00
command: 20 00 00 00
#
name: JOG_REVERSE_-
type: parsed
protocol: NECext
address: A8 00 00 00
command: 24 00 00 00
#
name: SHUT.FWD(FULL_SP)
type: parsed
protocol: NECext
address: A8 00 00 00
command: 2B 00 00 00
#
name: SHUT.REV(FULL_SP)
type: parsed
protocol: NECext
address: A8 00 00 00
command: 2F 00 00 00
#
name: D-LEVEL_CONTROL
type: parsed
protocol: NECext
address: A8 00 00 00
command: 37 00 00 00
#
name: ON_SCREEN
type: parsed
protocol: NECext
address: A8 00 00 00
command: 43 00 00 00
#
name: REPEAT_B
type: parsed
protocol: NECext
address: A8 00 00 00
command: 44 00 00 00
#
name: C_(CLEAR)
type: parsed
protocol: NECext
address: A8 00 00 00
command: 45 00 00 00
#
name: MULTI_SPEED_-
type: parsed
protocol: NECext
address: A8 00 00 00
command: 46 00 00 00
#
name: MULTI_SPEED_+
type: parsed
protocol: NECext
address: A8 00 00 00
command: 47 00 00 00
#
name: REPEAT_A
type: parsed
protocol: NECext
address: A8 00 00 00
command: 48 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: A8 00 00 00
command: 4C 00 00 00
#
name: DISC_SIDE_A
type: parsed
protocol: NECext
address: A8 00 00 00
command: 4D 00 00 00
#
name: DISC_SIDE_B
type: parsed
protocol: NECext
address: A8 00 00 00
command: 4E 00 00 00
#
name: STILL/STEP_<
type: parsed
protocol: NECext
address: A8 00 00 00
command: 50 00 00 00
#
name: SKIP_>>
type: parsed
protocol: NECext
address: A8 00 00 00
command: 52 00 00 00
#
name: SKIP_<<
type: parsed
protocol: NECext
address: A8 00 00 00
command: 53 00 00 00
#
name: STILL/STEP_>
type: parsed
protocol: NECext
address: A8 00 00 00
command: 54 00 00 00
#
name: MULTI_SPEED_<
type: parsed
protocol: NECext
address: A8 00 00 00
command: 55 00 00 00
#
name: MULTI_SPEED_>
type: parsed
protocol: NECext
address: A8 00 00 00
command: 58 00 00 00
#
name: HILITE/INTRO
type: parsed
protocol: NECext
address: A8 00 00 00
command: 5A 00 00 00
#
name: STROBE
type: parsed
protocol: NECext
address: A8 00 00 00
command: 5B 00 00 00
#
name: ONE_SHOT_MEMORY
type: parsed
protocol: NECext
address: A8 00 00 00
command: 5D 00 00 00
