Filetype: IR signals file
Version: 1
#
name: INTRO
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 46 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 81 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 84 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 85 00 00 00
#
name: PLAYPAUSE
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 87 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 8B 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 8F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 90 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 91 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 92 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 93 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 94 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 95 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 96 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 97 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 98 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 99 00 00 00
#
name: 102ND
type: parsed
protocol: NECext
address: A0 C2 00 00
command: 9F 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: A0 C2 00 00
command: A0 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: A0 C2 00 00
command: A2 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: A0 C2 00 00
command: A3 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: A0 C2 00 00
command: A6 00 00 00
#
name: RESET
type: parsed
protocol: NECext
address: A0 C2 00 00
command: AF 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: A0 C2 00 00
command: B0 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: A0 C2 00 00
command: B1 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: A0 C2 00 00
command: B8 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: A0 C2 00 00
command: BC 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: A0 C2 00 00
command: BD 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: A0 C2 00 00
command: BE 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: A0 C2 00 00
command: BF 00 00 00
#
name: SOUND
type: parsed
protocol: NECext
address: A0 C2 00 00
command: D9 00 00 00
#
name: VIRTUALIZER
type: parsed
protocol: NECext
address: A0 C2 00 00
command: DA 00 00 00
#
name: PAGEUP
type: parsed
protocol: NECext
address: A0 C2 00 00
command: E7 00 00 00
#
name: PAGEDOWN
type: parsed
protocol: NECext
address: A0 C2 00 00
command: E8 00 00 00
#
name: AUTOSCAN
type: parsed
protocol: NECext
address: A0 C2 00 00
command: EC 00 00 00
