Filetype: IR signals file
Version: 1
#
name: 6
type: parsed
protocol: NECext
address: 80 54 00 00
command: 00 00 00 00
#
name: DISPLAY/POWER
type: parsed
protocol: NECext
address: 80 54 00 00
command: 01 00 00 00
#
name: DISPLAY/MUTE
type: parsed
protocol: NECext
address: 80 54 00 00
command: 02 00 00 00
#
name: RGB/MUTE
type: parsed
protocol: NECext
address: 80 54 00 00
command: 03 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 80 54 00 00
command: 07 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 80 54 00 00
command: 08 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 80 54 00 00
command: 09 00 00 00
#
name: AUDIO/MUTE
type: parsed
protocol: NECext
address: 80 54 00 00
command: 0A 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 80 54 00 00
command: 0C 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 80 54 00 00
command: 0D 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 80 54 00 00
command: 0E 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 80 54 00 00
command: 11 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 80 54 00 00
command: 12 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 80 54 00 00
command: 15 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 80 54 00 00
command: 18 00 00 00
#
name: FUNCTION
type: parsed
protocol: NECext
address: 80 54 00 00
command: 19 00 00 00
