Filetype: IR signals file
Version: 1
# 
# Micca N8 Picture Frame
# 
name: POWER
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0D 00 00 00
# 
name: BGM
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0E 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0F 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
# 
name: Back
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0B 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0A 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 00 00 00 00
command: 16 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 00 00 00 00
command: 11 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 00 00 00 00
command: 13 00 00 00
# 
name: Setup
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
# 
name: Play
type: parsed
protocol: NEC
address: 00 00 00 00
command: 17 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 00 00 00 00
command: 19 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1A 00 00 00
# 
name: Zoom
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1B 00 00 00
# 
name: Reverse
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1D 00 00 00
# 
name: Foward
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1E 00 00 00
# 
name: Rotate
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1F 00 00 00
# 
name: Ok
type: parsed
protocol: NEC
address: 00 00 00 00
command: 12 00 00 00
