Filetype: IR signals file
Version: 1
#
name: 4
type: parsed
protocol: NECext
address: 86 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 86 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 86 00 00 00
command: 02 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 86 00 00 00
command: 03 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 86 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 86 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 86 00 00 00
command: 06 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 86 00 00 00
command: 07 00 00 00
#
name: TB
type: parsed
protocol: NECext
address: 86 00 00 00
command: 08 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 86 00 00 00
command: 09 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 86 00 00 00
command: 0A 00 00 00
#
name: TV/SAT
type: parsed
protocol: NECext
address: 86 00 00 00
command: 0B 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 86 00 00 00
command: 0C 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 86 00 00 00
command: 0D 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 86 00 00 00
command: 0F 00 00 00
#
name: VOL
type: parsed
protocol: NECext
address: 86 00 00 00
command: 10 00 00 00
#
name: CH_DN
type: parsed
protocol: NECext
address: 86 00 00 00
command: 11 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 86 00 00 00
command: 12 00 00 00
#
name: FREQ
type: parsed
protocol: NECext
address: 86 00 00 00
command: 13 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 86 00 00 00
command: 14 00 00 00
#
name: PC
type: parsed
protocol: NECext
address: 86 00 00 00
command: 15 00 00 00
#
name: PE
type: parsed
protocol: NECext
address: 86 00 00 00
command: 16 00 00 00
#
name: OFFSET
type: parsed
protocol: NECext
address: 86 00 00 00
command: 17 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 86 00 00 00
command: 19 00 00 00
#
name: H/V
type: parsed
protocol: NECext
address: 86 00 00 00
command: 1B 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 86 00 00 00
command: 1C 00 00 00
#
name: 2KHZ
type: parsed
protocol: NECext
address: 86 00 00 00
command: 1D 00 00 00
#
name: MEM
type: parsed
protocol: NECext
address: 86 00 00 00
command: 1E 00 00 00
#
name: LNB_A/B
type: parsed
protocol: NECext
address: 86 00 00 00
command: 1F 00 00 00
