Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 09 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 0A 00 00 00
#
name: minmax
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 0B 00 00 00
#
name: tv/av
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 0C 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 0E 00 00 00
#
name: TimeShift
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 0F 00 00 00
#
name: arrow_right
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 10 00 00 00
#
name: arrow_left
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 11 00 00 00
#
name: arrow_up
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 12 00 00 00
#
name: arrow_down
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 13 00 00 00
#
name: F11
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 14 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 15 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 16 00 00 00
#
name: Snapshot
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 17 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 18 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 19 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 1A 00 00 00
#
name: ESC
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 1C 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 1E 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 1F 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 40 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 41 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 42 00 00 00
#
name: click
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 43 00 00 00
#
name: Shuffle
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 44 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 02 BD 00 00
command: 45 00 00 00
