Filetype: IR signals file
Version: 1
# 
name: VOL+
type: parsed
protocol: RC5
address: 10 00 00 00
command: 10 00 00 00
# 
name: VOL-
type: parsed
protocol: RC5
address: 10 00 00 00
command: 11 00 00 00
# 
name: MUTE
type: parsed
protocol: RC5
address: 10 00 00 00
command: 0D 00 00 00
# 
name: Source
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 29 00 00 00
# 
name: Back
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 08 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 23 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 24 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 30 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 32 00 00 00
# 
name: Enter
type: parsed
protocol: NEC
address: 6E 00 00 00
command: 03 00 00 00
