Filetype: IR signals file
Version: 1
#
name: TELEPHOTO
type: parsed
protocol: NECext
address: D9 00 00 00
command: 1A 00 00 00
#
name: WIDE_ANGLE
type: parsed
protocol: NECext
address: D9 00 00 00
command: 1B 00 00 00
