Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: 102ND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: Colour
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: P.size
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 26 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: TTX/MIX
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
#
name: CH/P+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 50 00 00 00
#
name: CH/P-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 51 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 55 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 56 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 00 00 00 00
command: 6B 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 6C 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 6D 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 6E 00 00 00
