Filetype: IR signals file
Version: 1
#
name: fm/am
type: parsed
protocol: NECext
address: 02 02 00 00
command: 00 00 00 00
#
name: rds
type: parsed
protocol: NECext
address: 02 02 00 00
command: 01 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 02 02 00 00
command: 02 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 02 02 00 00
command: 03 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 02 02 00 00
command: 04 00 00 00
#
name: mdrec
type: parsed
protocol: NECext
address: 02 02 00 00
command: 05 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 02 02 00 00
command: 06 00 00 00
#
name: EDIT
type: parsed
protocol: NECext
address: 02 02 00 00
command: 07 00 00 00
#
name: EDIT
type: parsed
protocol: NECext
address: 02 02 00 00
command: 07 00 00 00
#
name: TAPE
type: parsed
protocol: NECext
address: 02 02 00 00
command: 08 00 00 00
#
name: pty
type: parsed
protocol: NECext
address: 02 02 00 00
command: 09 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 02 02 00 00
command: 0A 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 02 02 00 00
command: 0B 00 00 00
#
name: +100
type: parsed
protocol: NECext
address: 02 02 00 00
command: 0C 00 00 00
#
name: pickrec
type: parsed
protocol: NECext
address: 02 02 00 00
command: 0D 00 00 00
#
name: revmode
type: parsed
protocol: NECext
address: 02 02 00 00
command: 0E 00 00 00
#
name: editcancel
type: parsed
protocol: NECext
address: 02 02 00 00
command: 0F 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: 02 02 00 00
command: 10 00 00 00
#
name: ct
type: parsed
protocol: NECext
address: 02 02 00 00
command: 11 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 02 02 00 00
command: 12 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 02 02 00 00
command: 13 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 02 02 00 00
command: 14 00 00 00
#
name: checkspace
type: parsed
protocol: NECext
address: 02 02 00 00
command: 15 00 00 00
#
name: dolby
type: parsed
protocol: NECext
address: 02 02 00 00
command: 16 00 00 00
#
name: prog
type: parsed
protocol: NECext
address: 02 02 00 00
command: 17 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: 02 02 00 00
command: 18 00 00 00
#
name: rt
type: parsed
protocol: NECext
address: 02 02 00 00
command: 19 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 02 02 00 00
command: 1A 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 02 02 00 00
command: 1B 00 00 00
#
name: timer
type: parsed
protocol: NECext
address: 02 02 00 00
command: 1C 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 02 02 00 00
command: 1D 00 00 00
#
name: titleinput
type: parsed
protocol: NECext
address: 02 02 00 00
command: 1E 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 02 02 00 00
command: 1F 00 00 00
#
name: md
type: parsed
protocol: NECext
address: 02 02 00 00
command: 40 00 00 00
#
name: fmmode
type: parsed
protocol: NECext
address: 02 02 00 00
command: 41 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 02 02 00 00
command: 42 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 02 02 00 00
command: 43 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 02 02 00 00
command: 44 00 00 00
#
name: set
type: parsed
protocol: NECext
address: 02 02 00 00
command: 45 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 02 02 00 00
command: 46 00 00 00
#
name: 5modesrs
type: parsed
protocol: NECext
address: 02 02 00 00
command: 47 00 00 00
#
name: titlesearch
type: parsed
protocol: NECext
address: 02 02 00 00
command: 48 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 02 02 00 00
command: 49 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 02 02 00 00
command: 4A 00 00 00
#
name: random
type: parsed
protocol: NECext
address: 02 02 00 00
command: 4B 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 02 02 00 00
command: 4C 00 00 00
#
name: timedisp
type: parsed
protocol: NECext
address: 02 02 00 00
command: 4D 00 00 00
#
name: eqmode
type: parsed
protocol: NECext
address: 02 02 00 00
command: 4E 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 02 02 00 00
command: 4F 00 00 00
#
name: bass
type: parsed
protocol: NECext
address: 02 02 00 00
command: 50 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 02 02 00 00
command: 51 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 02 02 00 00
command: 52 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 02 02 00 00
command: 53 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 02 02 00 00
command: 56 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 02 02 00 00
command: 57 00 00 00
