Filetype: IR signals file
Version: 1
#
name: ^
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: ^_(CHANNEL)
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: CHANNEL_^
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: CH^
type: parsed
protocol: NECext
address: 04 00 00 00
command: 00 00 00 00
#
name: V
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: V_(CHANNEL)
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: CHANNEL_V
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: CHV
type: parsed
protocol: NECext
address: 04 00 00 00
command: 01 00 00 00
#
name: VOL_^
type: parsed
protocol: NECext
address: 04 00 00 00
command: 02 00 00 00
#
name: VOL^
type: parsed
protocol: NECext
address: 04 00 00 00
command: 02 00 00 00
#
name: VOL_V
type: parsed
protocol: NECext
address: 04 00 00 00
command: 03 00 00 00
#
name: VOLV
type: parsed
protocol: NECext
address: 04 00 00 00
command: 03 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 08 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 04 00 00 00
command: 09 00 00 00
#
name: ANT_A/B
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0A 00 00 00
#
name: OFF_TIMER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 0E 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 04 00 00 00
command: 10 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 04 00 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 04 00 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 04 00 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 04 00 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 04 00 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 04 00 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 04 00 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 04 00 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 04 00 00 00
command: 19 00 00 00
#
name: QUICK_VIEW
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1A 00 00 00
#
name: OFF_TIMER
type: parsed
protocol: NECext
address: 04 00 00 00
command: 1B 00 00 00
