Filetype: IR signals file
Version: 1
# 
# Canon Camera JJC RM-E6A
# Camera needs to be in IR remote control drive mode
#
name: Shutter
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 594 7182 593
# 
name: 2sec_Shutter
type: raw
frequency: 38000
duty_cycle: 0.330000
data: 566 5044 561
