Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: 102ND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: OFF
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: PP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: VOL_p
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: VOL+m
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 20 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 21 00 00 00
#
name: PlP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 22 00 00 00
#
name: i-ii
type: parsed
protocol: NECext
address: 00 00 00 00
command: 23 00 00 00
#
name: C
type: parsed
protocol: NECext
address: 00 00 00 00
command: 29 00 00 00
#
name: B
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2A 00 00 00
#
name: F
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2B 00 00 00
#
name: G
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2C 00 00 00
#
name: D
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2D 00 00 00
#
name: E
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2E 00 00 00
#
name: H
type: parsed
protocol: NECext
address: 00 00 00 00
command: 2F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 30 00 00 00
#
name: feature
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: install
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: picture
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: sound
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: Y
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: A
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3C 00 00 00
#
name: X
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
