Filetype: IR signals file
Version: 1
#
name: TV_VCR
type: parsed
protocol: NECext
address: 05 05 00 00
command: 01 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 05 05 00 00
command: 02 00 00 00
#
name: A.REP
type: parsed
protocol: NECext
address: 05 05 00 00
command: 03 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 05 05 00 00
command: 14 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 05 05 00 00
command: 15 00 00 00
#
name: P/S_N.C
type: parsed
protocol: NECext
address: 05 05 00 00
command: 16 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 05 05 00 00
command: 18 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 05 05 00 00
command: 19 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 05 05 00 00
command: 1A 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 05 05 00 00
command: 20 00 00 00
#
name: A.TRK
type: parsed
protocol: NECext
address: 05 05 00 00
command: 21 00 00 00
#
name: TRACKING__Up
type: parsed
protocol: NECext
address: 05 05 00 00
command: 2C 00 00 00
#
name: TRACKING_Down
type: parsed
protocol: NECext
address: 05 05 00 00
command: 2D 00 00 00
#
name: SYSTEM
type: parsed
protocol: NECext
address: 05 05 00 00
command: 32 00 00 00
