Filetype: IR signals file
Version: 1
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: M/P
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: TV/SAT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: TV/RAD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1A 00 00 00
#
name: I/O
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 41 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 42 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 43 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 44 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 45 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 46 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 47 00 00 00
#
name: Timer
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4B 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4F 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 50 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 53 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 57 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5B 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5E 00 00 00
