Filetype: IR signals file
Version: 1
#
name: MUTE
type: parsed
protocol: NECext
address: 0F 00 00 00
command: 3F 00 00 00
#
name: INPUT
type: parsed
protocol: NECext
address: 0F 00 00 00
command: A3 00 00 00
