Filetype: IR signals file
Version: 1
#
# ContinentalEdison CELED32JBL7 TV
# 
name: Power
type: parsed
protocol: NEC
address: 40 00 00 00
command: 0B 00 00 00
# 
name: Source
type: parsed
protocol: NEC
address: 40 00 00 00
command: 0F 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 40 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 40 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 40 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 40 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 40 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 40 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 40 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 40 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 40 00 00 00
command: 09 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 40 00 00 00
command: 00 00 00 00
# 
name: Ok
type: parsed
protocol: NEC
address: 40 00 00 00
command: 2F 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 40 00 00 00
command: 2B 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 40 00 00 00
command: 2C 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 40 00 00 00
command: 2E 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 40 00 00 00
command: 2D 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: 40 00 00 00
command: 15 00 00 00
# 
name: Exit
type: parsed
protocol: NEC
address: 40 00 00 00
command: 30 00 00 00
# 
name: Ch+
type: parsed
protocol: NEC
address: 40 00 00 00
command: 11 00 00 00
# 
name: Ch-
type: parsed
protocol: NEC
address: 40 00 00 00
command: 10 00 00 00
# 
name: Vol+
type: parsed
protocol: NEC
address: 40 00 00 00
command: 13 00 00 00
# 
name: Vol-
type: parsed
protocol: NEC
address: 40 00 00 00
command: 12 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 40 00 00 00
command: 14 00 00 00
# 
name: Info
type: parsed
protocol: NEC
address: 40 00 00 00
command: 0A 00 00 00
