Filetype: IR signals file
Version: 1
#
name: KPPLUS
type: parsed
protocol: NECext
address: 31 00 00 00
command: 01 00 00 00
#
name: KPMINUS
type: parsed
protocol: NECext
address: 31 00 00 00
command: 02 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 31 00 00 00
command: 04 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 31 00 00 00
command: 05 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 31 00 00 00
command: 06 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 31 00 00 00
command: 07 00 00 00
#
name: TV/VCR
type: parsed
protocol: NECext
address: 31 00 00 00
command: 08 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 31 00 00 00
command: 0C 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 31 00 00 00
command: 0D 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 31 00 00 00
command: 0E 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 31 00 00 00
command: 0F 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 31 00 00 00
command: 10 00 00 00
#
name: PAUSE/STILL
type: parsed
protocol: NECext
address: 31 00 00 00
command: 11 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 31 00 00 00
command: 12 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 31 00 00 00
command: 13 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 31 00 00 00
command: 14 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 31 00 00 00
command: 15 00 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: 31 00 00 00
command: 1A 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 31 00 00 00
command: 1C 00 00 00
#
name: 0/AV
type: parsed
protocol: NECext
address: 31 00 00 00
command: 1D 00 00 00
#
name: ATR
type: parsed
protocol: NECext
address: 31 00 00 00
command: 1F 00 00 00
#
name: MEMORY
type: parsed
protocol: NECext
address: 31 00 00 00
command: 43 00 00 00
#
name: RESET
type: parsed
protocol: NECext
address: 31 00 00 00
command: 44 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 31 00 00 00
command: 4B 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: 31 00 00 00
command: 4C 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 31 00 00 00
command: 5B 00 00 00
#
name: SP/LP
type: parsed
protocol: NECext
address: 31 00 00 00
command: 5E 00 00 00
#
name: SHOW_VIEW
type: parsed
protocol: NECext
address: 31 00 00 00
command: 8C 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 31 00 00 00
command: 94 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 31 00 00 00
command: 95 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 31 00 00 00
command: 96 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 31 00 00 00
command: 97 00 00 00
#
name: MENU/TV
type: parsed
protocol: NECext
address: 31 00 00 00
command: CA 00 00 00
