Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 00 49 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 49 00 00
command: 03 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 49 00 00
command: 04 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 49 00 00
command: 05 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 49 00 00
command: 06 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 49 00 00
command: 07 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 49 00 00
command: 08 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 49 00 00
command: 09 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 49 00 00
command: 0A 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 49 00 00
command: 0B 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 49 00 00
command: 0C 00 00 00
#
name: MENY
type: parsed
protocol: NECext
address: 00 49 00 00
command: 0E 00 00 00
#
name: P-
type: parsed
protocol: NECext
address: 00 49 00 00
command: 0F 00 00 00
#
name: P+
type: parsed
protocol: NECext
address: 00 49 00 00
command: 10 00 00 00
#
name: CURSOR_UP
type: parsed
protocol: NECext
address: 00 49 00 00
command: 11 00 00 00
#
name: CURSOR_LEFT
type: parsed
protocol: NECext
address: 00 49 00 00
command: 12 00 00 00
#
name: CURSOR_OK
type: parsed
protocol: NECext
address: 00 49 00 00
command: 13 00 00 00
#
name: CURSOR_RIGHT
type: parsed
protocol: NECext
address: 00 49 00 00
command: 14 00 00 00
#
name: CURSOR_DOWN
type: parsed
protocol: NECext
address: 00 49 00 00
command: 15 00 00 00
#
name: BACK
type: parsed
protocol: NECext
address: 00 49 00 00
command: 16 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 49 00 00
command: 18 00 00 00
#
name: RG_GUL
type: parsed
protocol: NECext
address: 00 49 00 00
command: 1A 00 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 00 49 00 00
command: 1B 00 00 00
#
name: D
type: parsed
protocol: NECext
address: 00 49 00 00
command: 1C 00 00 00
#
name: N
type: parsed
protocol: NECext
address: 00 49 00 00
command: 1D 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 00 49 00 00
command: 1E 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 49 00 00
command: 1F 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 49 00 00
command: 40 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 00 49 00 00
command: 41 00 00 00
#
name: OPT+
type: parsed
protocol: NECext
address: 00 49 00 00
command: 42 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 49 00 00
command: 43 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 00 49 00 00
command: 46 00 00 00
#
name: PAGE+
type: parsed
protocol: NECext
address: 00 49 00 00
command: 49 00 00 00
#
name: PAGE-
type: parsed
protocol: NECext
address: 00 49 00 00
command: 4A 00 00 00
#
name: LIST
type: parsed
protocol: NECext
address: 00 49 00 00
command: 4D 00 00 00
#
name: WIDE
type: parsed
protocol: NECext
address: 00 49 00 00
command: 4E 00 00 00
#
name: V-FORMAT
type: parsed
protocol: NECext
address: 00 49 00 00
command: 4F 00 00 00
