Filetype: IR signals file
Version: 1
# 
# Telefunken_L65F249i3C
#
name: POWER
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0C 00 00 00
# 
name: 1
type: parsed
protocol: RC5
address: 01 00 00 00
command: 01 00 00 00
# 
name: 2
type: parsed
protocol: RC5
address: 01 00 00 00
command: 02 00 00 00
# 
name: 3
type: parsed
protocol: RC5
address: 01 00 00 00
command: 03 00 00 00
# 
name: 4
type: parsed
protocol: RC5
address: 01 00 00 00
command: 04 00 00 00
# 
name: 5
type: parsed
protocol: RC5
address: 01 00 00 00
command: 05 00 00 00
# 
name: 6
type: parsed
protocol: RC5
address: 01 00 00 00
command: 06 00 00 00
# 
name: 7
type: parsed
protocol: RC5
address: 01 00 00 00
command: 07 00 00 00
# 
name: 8
type: parsed
protocol: RC5
address: 01 00 00 00
command: 08 00 00 00
# 
name: 9
type: parsed
protocol: RC5
address: 01 00 00 00
command: 09 00 00 00
# 
name: 0
type: parsed
protocol: RC5
address: 01 00 00 00
command: 00 00 00 00
# 
name: MUTE
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0D 00 00 00
# 
name: VOL+
type: parsed
protocol: RC5
address: 01 00 00 00
command: 10 00 00 00
# 
name: VOL-
type: parsed
protocol: RC5
address: 01 00 00 00
command: 11 00 00 00
# 
name: CH+
type: parsed
protocol: RC5
address: 01 00 00 00
command: 20 00 00 00
# 
name: CH-
type: parsed
protocol: RC5
address: 01 00 00 00
command: 21 00 00 00
# 
name: Smart_Tv
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2E 00 00 00
# 
name: Menu
type: parsed
protocol: RC5
address: 01 00 00 00
command: 30 00 00 00
# 
name: Eco_Menu
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2B 00 00 00
# 
name: Up
type: parsed
protocol: RC5
address: 01 00 00 00
command: 14 00 00 00
# 
name: Down
type: parsed
protocol: RC5
address: 01 00 00 00
command: 13 00 00 00
# 
name: Left
type: parsed
protocol: RC5
address: 01 00 00 00
command: 15 00 00 00
# 
name: Right
type: parsed
protocol: RC5
address: 01 00 00 00
command: 16 00 00 00
# 
name: Back
type: parsed
protocol: RC5
address: 01 00 00 00
command: 0A 00 00 00
# 
name: Exit
type: parsed
protocol: RC5
address: 01 00 00 00
command: 25 00 00 00
# 
name: Ok_enter
type: parsed
protocol: RC5
address: 01 00 00 00
command: 35 00 00 00
# 
name: Info
type: parsed
protocol: RC5
address: 01 00 00 00
command: 12 00 00 00
# 
name: Mediabrowser
type: parsed
protocol: RC5
address: 01 00 00 00
command: 39 00 00 00
# 
name: Teletext
type: parsed
protocol: RC5
address: 01 00 00 00
command: 2F 00 00 00
# 
name: Play
type: parsed
protocol: RC5
address: 01 00 00 00
command: 19 00 00 00
# 
name: Pause
type: parsed
protocol: RC5
address: 01 00 00 00
command: 31 00 00 00
# 
name: Skip_Forward
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1C 00 00 00
# 
name: Skip_Back
type: parsed
protocol: RC5
address: 01 00 00 00
command: 1B 00 00 00
