Filetype: IR signals file
Version: 1
#
name: pip
type: parsed
protocol: NECext
address: 61 63 00 00
command: 00 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 61 63 00 00
command: 01 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 61 63 00 00
command: 02 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 61 63 00 00
command: 03 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 61 63 00 00
command: 04 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 61 63 00 00
command: 05 00 00 00
#
name: display
type: parsed
protocol: NECext
address: 61 63 00 00
command: 06 00 00 00
#
name: wide
type: parsed
protocol: NECext
address: 61 63 00 00
command: 07 00 00 00
#
name: active
type: parsed
protocol: NECext
address: 61 63 00 00
command: 09 00 00 00
#
name: size
type: parsed
protocol: NECext
address: 61 63 00 00
command: 0B 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 61 63 00 00
command: 0C 00 00 00
#
name: position
type: parsed
protocol: NECext
address: 61 63 00 00
command: 0D 00 00 00
#
name: swap
type: parsed
protocol: NECext
address: 61 63 00 00
command: 0E 00 00 00
#
name: index
type: parsed
protocol: NECext
address: 61 63 00 00
command: 0F 00 00 00
#
name: sizemode
type: parsed
protocol: NECext
address: 61 63 00 00
command: 10 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 61 63 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 61 63 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 61 63 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 61 63 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 61 63 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 61 63 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 61 63 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 61 63 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 61 63 00 00
command: 19 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 61 63 00 00
command: 1A 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 61 63 00 00
command: 1C 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 61 63 00 00
command: 1E 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 61 63 00 00
command: 1F 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 61 63 00 00
command: 20 00 00 00
#
name: srs
type: parsed
protocol: NECext
address: 61 63 00 00
command: 21 00 00 00
#
name: av
type: parsed
protocol: NECext
address: 61 63 00 00
command: 22 00 00 00
#
name: scart
type: parsed
protocol: NECext
address: 61 63 00 00
command: 23 00 00 00
#
name: PC
type: parsed
protocol: NECext
address: 61 63 00 00
command: 24 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 61 63 00 00
command: 25 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 61 63 00 00
command: 26 00 00 00
#
name: mpx
type: parsed
protocol: NECext
address: 61 63 00 00
command: 27 00 00 00
#
name: mix
type: parsed
protocol: NECext
address: 61 63 00 00
command: 28 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 61 63 00 00
command: 29 00 00 00
#
name: RED
type: parsed
protocol: NECext
address: 61 63 00 00
command: 3A 00 00 00
#
name: GREEN
type: parsed
protocol: NECext
address: 61 63 00 00
command: 3B 00 00 00
#
name: YELLOW
type: parsed
protocol: NECext
address: 61 63 00 00
command: 3C 00 00 00
#
name: BLUE
type: parsed
protocol: NECext
address: 61 63 00 00
command: 3D 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 61 63 00 00
command: 40 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 61 63 00 00
command: 41 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 61 63 00 00
command: 42 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 61 63 00 00
command: 43 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 61 63 00 00
command: 44 00 00 00
#
name: hold
type: parsed
protocol: NECext
address: 61 63 00 00
command: 46 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 61 63 00 00
command: 49 00 00 00
#
name: TEXT
type: parsed
protocol: NECext
address: 61 63 00 00
command: 4A 00 00 00
#
name: reveal
type: parsed
protocol: NECext
address: 61 63 00 00
command: 4B 00 00 00
#
name: ebutton
type: parsed
protocol: NECext
address: 61 63 00 00
command: 65 00 00 00
