Filetype: IR signals file
Version: 1
# 
# Pyle 4 Channel Receiver P2203ABTU
#
name: POWER
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1C 00 00 00
# 
name: DVD_CD
type: parsed
protocol: NEC
address: 00 00 00 00
command: 19 00 00 00
# 
name: TUNER
type: parsed
protocol: NEC
address: 00 00 00 00
command: 40 00 00 00
# 
name: BT_USB
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1D 00 00 00
# 
name: IPOD_MP3
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1B 00 00 00
# 
name: VOL+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0F 00 00 00
# 
name: VOL-
type: parsed
protocol: NEC
address: 00 00 00 00
command: 05 00 00 00
# 
name: LEFT
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0A 00 00 00
# 
name: RIGHT
type: parsed
protocol: NEC
address: 00 00 00 00
command: 09 00 00 00
# 
name: TREBLE-
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0E 00 00 00
# 
name: TREBLE+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 08 00 00 00
# 
name: BASS_
type: parsed
protocol: NEC
address: 00 00 00 00
command: 06 00 00 00
# 
name: BASS+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 04 00 00 00
# 
name: MUTE
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0B 00 00 00
# 
name: SPEAK_A
type: parsed
protocol: NEC
address: 00 00 00 00
command: 59 00 00 00
# 
name: SPEAK_B
type: parsed
protocol: NEC
address: 00 00 00 00
command: 43 00 00 00
# 
name: SPEAK_A+B
type: parsed
protocol: NEC
address: 00 00 00 00
command: 46 00 00 00
# 
name: LOUD
type: parsed
protocol: NEC
address: 00 00 00 00
command: 47 00 00 00
# 
name: DIP_1
type: parsed
protocol: NEC
address: 00 00 00 00
command: 44 00 00 00
# 
name: DSP_2
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4C 00 00 00
# 
name: DSP_3
type: parsed
protocol: NEC
address: 00 00 00 00
command: 00 00 00 00
# 
name: DSP_4
type: parsed
protocol: NEC
address: 00 00 00 00
command: 07 00 00 00
# 
name: DSP_5
type: parsed
protocol: NEC
address: 00 00 00 00
command: 11 00 00 00
# 
name: DSP_6
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1A 00 00 00
# 
name: DSP_7
type: parsed
protocol: NEC
address: 00 00 00 00
command: 12 00 00 00
# 
name: OFF
type: parsed
protocol: NEC
address: 00 00 00 00
command: 55 00 00 00
# 
name: AUTO_SCAN
type: parsed
protocol: NEC
address: 00 00 00 00
command: 5C 00 00 00
# 
name: AM
type: parsed
protocol: NEC
address: 00 00 00 00
command: 03 00 00 00
# 
name: FM
type: parsed
protocol: NEC
address: 00 00 00 00
command: 02 00 00 00
# 
name: VFD+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 01 00 00 00
# 
name: VFD-
type: parsed
protocol: NEC
address: 00 00 00 00
command: 58 00 00 00
# 
name: MEMORY
type: parsed
protocol: NEC
address: 00 00 00 00
command: 45 00 00 00
# 
name: PREV
type: parsed
protocol: NEC
address: 00 00 00 00
command: 4D 00 00 00
# 
name: NEXT
type: parsed
protocol: NEC
address: 00 00 00 00
command: 54 00 00 00
# 
name: ST_MONO
type: parsed
protocol: NEC
address: 00 00 00 00
command: 5E 00 00 00
# 
name: TUNING-
type: parsed
protocol: NEC
address: 00 00 00 00
command: 50 00 00 00
# 
name: TUNING+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 49 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 00 00 00 00
command: 18 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1F 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 00 00 00 00
command: 1E 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 00 00 00 00
command: 14 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 00 00 00 00
command: 15 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 00 00 00 00
command: 10 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 00 00 00 00
command: 17 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 00 00 00 00
command: 16 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 00 00 00 00
command: 13 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0C 00 00 00
# 
name: 10+
type: parsed
protocol: NEC
address: 00 00 00 00
command: 0D 00 00 00