Filetype: IR signals file
Version: 1
#
# YAMAHA RAX21
# Autogenerated from ircodes/YAMAHA (AVR Stereo)/RAX21.xml
#
name: POWER
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 0F F0 00 00
#
name: iPOD
type: parsed
protocol: NECext
address: E1 1E 00 00
command: F4 0B 00 00
#
name: CD
type: parsed
protocol: NECext
address: E1 1E 00 00
command: AD 52 00 00
#
name: USB
type: parsed
protocol: NECext
address: E1 1E 00 00
command: C2 3D 00 00
#
name: FM/AM
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 2D D2 00 00
#
name: PHONO
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 6D 92 00 00
#
name: AUX
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 84 7B 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: E1 1E 00 00
command: C7 38 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 27 D8 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 6A 95 00 00
#
name: MEMORY
type: parsed
protocol: NECext
address: E1 1E 00 00
command: B2 4D 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: E1 1E 00 00
command: AA 55 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: E1 1E 00 00
command: CF 30 00 00
#
name: STOP
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 7F 80 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 1F E0 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 01 FE 00 00
command: D7 28 00 00
#
name: iPod MENU SEL
type: parsed
protocol: NECext
address: 01 FE 00 00
command: EE 11 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 01 FE 00 00
command: 8F 70 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 01 FE 00 00
command: 0F F0 00 00
#
name: PREV
type: parsed
protocol: NECext
address: 01 FE 00 00
command: 27 D8 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 01 FE 00 00
command: 77 88 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 01 FE 00 00
command: C7 38 00 00
#
name: /
type: parsed
protocol: NECext
address: 01 FE 00 00
command: 87 78 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 07 F8 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 87 78 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 95 6A 00 00
#
name: TONE/BALANCE
type: parsed
protocol: NECext
address: E1 1E 00 00
command: DE 21 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 55 AA 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: E1 1E 00 00
command: AF 50 00 00
#
name: DIMMER
type: parsed
protocol: NECext
address: E1 1E 00 00
command: A2 5D 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: E1 1E 00 00
command: 0D F2 00 00
#
name: PURE DIRECT
type: parsed
protocol: NECext
address: E1 1E 00 00
command: F5 0A 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: E1 1E 00 00
command: C6 39 00 00
