Filetype: IR signals file
Version: 1
#
name: FORWARD
type: parsed
protocol: NECext
address: 89 77 00 00
command: 01 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 89 77 00 00
command: 02 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 89 77 00 00
command: 03 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 89 77 00 00
command: 06 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 89 77 00 00
command: 07 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 89 77 00 00
command: 08 00 00 00
#
name: STILL
type: parsed
protocol: NECext
address: 89 77 00 00
command: 09 00 00 00
#
name: RESET
type: parsed
protocol: NECext
address: 89 77 00 00
command: 0A 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 89 77 00 00
command: 0D 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 89 77 00 00
command: 0E 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 89 77 00 00
command: 0F 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 89 77 00 00
command: 10 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 89 77 00 00
command: 13 00 00 00
#
name: F11
type: parsed
protocol: NECext
address: 89 77 00 00
command: 14 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 89 77 00 00
command: 16 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 89 77 00 00
command: 17 00 00 00
#
name: AUTO
type: parsed
protocol: NECext
address: 89 77 00 00
command: 18 00 00 00
#
name: SPEED_UP
type: parsed
protocol: NECext
address: 89 77 00 00
command: 1A 00 00 00
#
name: SPEED_DOWN
type: parsed
protocol: NECext
address: 89 77 00 00
command: 1B 00 00 00
#
name: VID_MODE
type: parsed
protocol: NECext
address: 89 77 00 00
command: 4E 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 89 77 00 00
command: 50 00 00 00
#
name: DIMMER
type: parsed
protocol: NECext
address: 89 77 00 00
command: 51 00 00 00
#
name: TIMER
type: parsed
protocol: NECext
address: 89 77 00 00
command: 53 00 00 00
#
name: PROG_LIST
type: parsed
protocol: NECext
address: 89 77 00 00
command: 54 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 89 77 00 00
command: 55 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: 89 77 00 00
command: 56 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 89 77 00 00
command: 58 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 89 77 00 00
command: 59 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 89 77 00 00
command: 5C 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 89 77 00 00
command: 5D 00 00 00
#
name: PROG
type: parsed
protocol: NECext
address: 89 77 00 00
command: 5F 00 00 00
