Filetype: IR signals file
Version: 1
#
name: TAPE_1/2_PLAY
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 00 00 00 00
#
name: TAPE_1/2_REWIND
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 01 00 00 00
#
name: TAPE_1/2_FAST_FWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 02 00 00 00
#
name: TAPE_1/2_STOP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 03 00 00 00
#
name: TAPE_1/2_REC/PAUSE
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 04 00 00 00
#
name: TAPE_1/2_RECORD_MUTE
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 05 00 00 00
#
name: DECK_A/B
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 06 00 00 00
#
name: TAPE_1/2_DIR_A
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 07 00 00 00
#
name: CD_PLAY
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 08 00 00 00
#
name: CD_PAUSE/STOP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 09 00 00 00
#
name: CD_SKIP_FWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0A 00 00 00
#
name: CD_SKIP_REV
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0B 00 00 00
#
name: CD_SEARCH_FWD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0C 00 00 00
#
name: CD_SEARCH_REV
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0D 00 00 00
#
name: PHONO_PLAY/CUT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 0E 00 00 00
#
name: TUNER_PRESET_+
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 10 00 00 00
#
name: TUNER_PRESET_-
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 11 00 00 00
#
name: TUNER_A/B/C/D/E/
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 12 00 00 00
#
name: PHONO
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 14 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 15 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 16 00 00 00
#
name: AUX
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 17 00 00 00
#
name: TAPE_1/DAT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 18 00 00 00
#
name: TAPE_2
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 19 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1A 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 1B 00 00 00
#
name: TAPE_1/2_DIR_B
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 40 00 00 00
#
name: CD_DISK_SKIP
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 4F 00 00 00
#
name: EQ_ON/FLAT
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 5A 00 00 00
#
name: EQ_PRESET_+
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 5B 00 00 00
#
name: EQ_PRESET_-
type: parsed
protocol: NECext
address: 7A 00 00 00
command: 5C 00 00 00
