Filetype: IR signals file
Version: 1
#
name: STOP
type: parsed
protocol: NECext
address: 80 70 00 00
command: 01 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 80 70 00 00
command: 02 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 80 70 00 00
command: 03 00 00 00
#
name: <<SEARCH
type: parsed
protocol: NECext
address: 80 70 00 00
command: 06 00 00 00
#
name: SEARCH>>
type: parsed
protocol: NECext
address: 80 70 00 00
command: 06 00 00 00
#
name: REPEAT
type: parsed
protocol: NECext
address: 80 70 00 00
command: 0A 00 00 00
#
name: INTRO_SCAN
type: parsed
protocol: NECext
address: 80 70 00 00
command: 0D 00 00 00
#
name: PROGRAM
type: parsed
protocol: NECext
address: 80 70 00 00
command: 0E 00 00 00
#
name: CLEAR
type: parsed
protocol: NECext
address: 80 70 00 00
command: 0F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 80 70 00 00
command: 11 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 80 70 00 00
command: 12 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 80 70 00 00
command: 13 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 80 70 00 00
command: 14 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 80 70 00 00
command: 15 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 80 70 00 00
command: 16 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 80 70 00 00
command: 17 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 80 70 00 00
command: 18 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 80 70 00 00
command: 19 00 00 00
#
name: TIME
type: parsed
protocol: NECext
address: 80 70 00 00
command: 1C 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 80 70 00 00
command: 40 00 00 00
#
name: RANDOM
type: parsed
protocol: NECext
address: 80 70 00 00
command: 4D 00 00 00
#
name: SKIP_UP
type: parsed
protocol: NECext
address: 80 70 00 00
command: 50 00 00 00
#
name: DISC_1
type: parsed
protocol: NECext
address: 80 70 00 00
command: 51 00 00 00
#
name: DISC_2
type: parsed
protocol: NECext
address: 80 70 00 00
command: 52 00 00 00
#
name: DISC_3
type: parsed
protocol: NECext
address: 80 70 00 00
command: 53 00 00 00
#
name: DISC_4
type: parsed
protocol: NECext
address: 80 70 00 00
command: 54 00 00 00
#
name: DISC_5
type: parsed
protocol: NECext
address: 80 70 00 00
command: 55 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 80 70 00 00
command: 56 00 00 00
#
name: OFF
type: parsed
protocol: NECext
address: 80 70 00 00
command: 57 00 00 00
#
name: SKIP_DN
type: parsed
protocol: NECext
address: 80 70 00 00
command: 5B 00 00 00
