Filetype: IR signals file
Version: 1
# 
name: POWER
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: E6 00 00 00
# 
name: Source
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 01 00 00 00
# 
name: Up
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 60 00 00 00
# 
name: Down
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 61 00 00 00
# 
name: Left
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 65 00 00 00
# 
name: Right
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 62 00 00 00
# 
name: OK
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 68 00 00 00
# 
name: Return
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 58 00 00 00
# 
name: Exit
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 2D 00 00 00
# 
name: Home
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 79 00 00 00
# 
name: MUTE
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0F 00 00 00
# 
name: VolUp
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 07 00 00 00
# 
name: VolDown
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 0B 00 00 00
# 
name: ChanUp
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 12 00 00 00
# 
name: ChanDown
type: parsed
protocol: Samsung32
address: 07 00 00 00
command: 10 00 00 00
