Filetype: IR signals file
Version: 1
#
name: FC_SCAN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: FC_MEMO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: TV_/_CATV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: CHANNEL_-_PREVIOUS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 1--
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: CHANNEL_-_DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: CHANNEL_-_UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0D 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0E 00 00 00
#
name: VOL-_DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: VOL-_UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: PC
type: parsed
protocol: NECext
address: 00 00 00 00
command: 14 00 00 00
#
name: PC_MEMO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: PC_SCAN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 16 00 00 00
#
name: VOL-_MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: SLEEP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 18 00 00 00
#
name: MTS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1F 00 00 00
