Filetype: IR signals file
Version: 1
#
name: Jump
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: PLAYPAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: T/S
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1A 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 43 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 46 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4B 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4E 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4F 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 53 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 57 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 58 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 59 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5A 00 00 00
#
name: TV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5B 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5C 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5E 00 00 00
#
name: Input
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5F 00 00 00
