Filetype: IR signals file
Version: 1
#
name: RECORD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 00 00 00 00
#
name: turnup
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 01 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 01 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 02 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 02 00 00 00
#
name: tv/fm
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 03 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 03 00 00 00
#
name: fm-freq-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 04 00 00 00
#
name: function-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 04 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 04 00 00 00
#
name: function-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 04 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 05 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 06 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 06 00 00 00
#
name: CYCLEWINDOWS
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 07 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 07 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 08 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 08 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 09 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 09 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0A 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0A 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0B 00 00 00
#
name: EPG
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0B 00 00 00
#
name: fm_freq+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0C 00 00 00
#
name: function+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0C 00 00 00
#
name: scan
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0C 00 00 00
#
name: function+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0C 00 00 00
#
name: mts
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0D 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0D 00 00 00
#
name: function
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0E 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0E 00 00 00
#
name: minimze
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0F 00 00 00
#
name: CYCLEWINDOWS
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 0F 00 00 00
#
name: KPPLUS
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 10 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 10 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 11 00 00 00
#
name: REWIND
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 11 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 12 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 12 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 13 00 00 00
#
name: snap
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 13 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 14 00 00 00
#
name: pip
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 14 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 15 00 00 00
#
name: reset
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 15 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 16 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 16 00 00 00
#
name: fm_scan-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 17 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 17 00 00 00
#
name: turnleft
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 17 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 17 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 18 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 18 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 19 00 00 00
#
name: FORWARD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 19 00 00 00
#
name: snapshot
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1A 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1A 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1B 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1B 00 00 00
#
name: scan
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1C 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1C 00 00 00
#
name: reset
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1D 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1D 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1E 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1E 00 00 00
#
name: fm_scan+
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1F 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1F 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 86 6B 00 00
command: 1F 00 00 00
