Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: TAB
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK--
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK++
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK-
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK+
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: 10CHANNELSUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: MODE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: TAB
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: ZOOM
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: FREEZE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK--
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK++
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK-
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: SEEK+
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: EJECTCD
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F1
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F2
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F3
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: F4
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 3F 00 00 00
command: 3F 00 00 00
