Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: C1 44 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: C1 44 00 00
command: 09 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: C1 44 00 00
command: 11 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: C1 44 00 00
command: 1E 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: C1 44 00 00
command: 21 00 00 00
#
name: EAX
type: parsed
protocol: NECext
address: C1 44 00 00
command: 31 00 00 00
#
name: CANCEL
type: parsed
protocol: NECext
address: C1 44 00 00
command: 3E 00 00 00
#
name: OPTION
type: parsed
protocol: NECext
address: C1 44 00 00
command: 41 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: C1 44 00 00
command: 46 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: C1 44 00 00
command: 51 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: C1 44 00 00
command: 5E 00 00 00
#
name: Display
type: parsed
protocol: NECext
address: C1 44 00 00
command: 6E 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: C1 44 00 00
command: 71 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: C1 44 00 00
command: 76 00 00 00
#
name: Step
type: parsed
protocol: NECext
address: C1 44 00 00
command: 7E 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: C1 44 00 00
command: 81 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: C1 44 00 00
command: 86 00 00 00
#
name: CMSS
type: parsed
protocol: NECext
address: C1 44 00 00
command: 8E 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: C1 44 00 00
command: 91 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: C1 44 00 00
command: 9E 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: C1 44 00 00
command: A1 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: C1 44 00 00
command: AE 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: C1 44 00 00
command: B1 00 00 00
#
name: SLOW
type: parsed
protocol: NECext
address: C1 44 00 00
command: BE 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: C1 44 00 00
command: C1 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: C1 44 00 00
command: C6 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: C1 44 00 00
command: CE 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: C1 44 00 00
command: D1 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: C1 44 00 00
command: DE 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: C1 44 00 00
command: E1 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: C1 44 00 00
command: EE 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: C1 44 00 00
command: F1 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: C1 44 00 00
command: FE 00 00 00
