Filetype: IR signals file
Version: 1
#
name: REWIND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: Firefly
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: FASTFORWARD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0A 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0F 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: PREVIOUS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 17 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: NEXT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1F 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 40 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 41 00 00 00
#
name: CLOSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 43 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 44 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 45 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 47 00 00 00
#
name: OK
type: parsed
protocol: NECext
address: 00 00 00 00
command: 48 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 49 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4B 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4C 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4D 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 4F 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 50 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 51 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 53 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 00 00 00 00
command: 54 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 55 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 57 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 58 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 00 00 00 00
command: 59 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5B 00 00 00
#
name: OPTION
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5C 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5D 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 5F 00 00 00
