Filetype: IR signals file
Version: 1
#
name: CD_SCAN_<<
type: parsed
protocol: NECext
address: B8 00 00 00
command: 06 00 00 00
#
name: CD_SCAN_>>
type: parsed
protocol: NECext
address: B8 00 00 00
command: 07 00 00 00
#
name: CD_DISC
type: parsed
protocol: NECext
address: B8 00 00 00
command: 08 00 00 00
#
name: TUNER/CD_+10
type: parsed
protocol: NECext
address: B8 00 00 00
command: 0D 00 00 00
#
name: 10+
type: parsed
protocol: NECext
address: B8 00 00 00
command: 0D 00 00 00
#
name: EQ.EFFECT
type: parsed
protocol: NECext
address: B8 00 00 00
command: 0F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: B8 00 00 00
command: 1D 00 00 00
#
name: DELAY_TIME_V
type: parsed
protocol: NECext
address: B8 00 00 00
command: 4C 00 00 00
#
name: DELAY_TIME_DWN
type: parsed
protocol: NECext
address: B8 00 00 00
command: 4C 00 00 00
#
name: DELAY_TIME_^
type: parsed
protocol: NECext
address: B8 00 00 00
command: 4D 00 00 00
#
name: DELAY_TIME_UP
type: parsed
protocol: NECext
address: B8 00 00 00
command: 4D 00 00 00
#
name: TEST_TONE_ON/OFF
type: parsed
protocol: NECext
address: B8 00 00 00
command: 56 00 00 00
#
name: TEST_TONE_MODE
type: parsed
protocol: NECext
address: B8 00 00 00
command: 57 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: 58 00 00 00
#
name: VIDEO_4
type: parsed
protocol: NECext
address: B8 00 00 00
command: 59 00 00 00
#
name: TUNER/CD_0
type: parsed
protocol: NECext
address: B8 00 00 00
command: 80 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: B8 00 00 00
command: 80 00 00 00
#
name: TUNER/CD_1
type: parsed
protocol: NECext
address: B8 00 00 00
command: 81 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: B8 00 00 00
command: 81 00 00 00
#
name: TUNER/CD_2
type: parsed
protocol: NECext
address: B8 00 00 00
command: 82 00 00 00
#
name: TUNER/CD_3
type: parsed
protocol: NECext
address: B8 00 00 00
command: 83 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: B8 00 00 00
command: 83 00 00 00
#
name: TUNER/CD_4
type: parsed
protocol: NECext
address: B8 00 00 00
command: 84 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: B8 00 00 00
command: 84 00 00 00
#
name: TUNER/CD_5
type: parsed
protocol: NECext
address: B8 00 00 00
command: 85 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: B8 00 00 00
command: 85 00 00 00
#
name: TUNER/CD_6
type: parsed
protocol: NECext
address: B8 00 00 00
command: 86 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: B8 00 00 00
command: 86 00 00 00
#
name: TUNER/CD_7
type: parsed
protocol: NECext
address: B8 00 00 00
command: 87 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: B8 00 00 00
command: 87 00 00 00
#
name: TUNER/CD_8
type: parsed
protocol: NECext
address: B8 00 00 00
command: 88 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: B8 00 00 00
command: 88 00 00 00
#
name: TUNER/CD_9
type: parsed
protocol: NECext
address: B8 00 00 00
command: 89 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: B8 00 00 00
command: 89 00 00 00
#
name: VIDEO_3
type: parsed
protocol: NECext
address: B8 00 00 00
command: 8A 00 00 00
#
name: TUNER_P.CALL_V
type: parsed
protocol: NECext
address: B8 00 00 00
command: 8C 00 00 00
#
name: TUNER_DWN
type: parsed
protocol: NECext
address: B8 00 00 00
command: 8C 00 00 00
#
name: TUNER_BAND
type: parsed
protocol: NECext
address: B8 00 00 00
command: 8F 00 00 00
#
name: BAND
type: parsed
protocol: NECext
address: B8 00 00 00
command: 8F 00 00 00
#
name: PHONO
type: parsed
protocol: NECext
address: B8 00 00 00
command: 90 00 00 00
#
name: TUNER
type: parsed
protocol: NECext
address: B8 00 00 00
command: 91 00 00 00
#
name: CD
type: parsed
protocol: NECext
address: B8 00 00 00
command: 92 00 00 00
#
name: VIDEO_2
type: parsed
protocol: NECext
address: B8 00 00 00
command: 93 00 00 00
#
name: TAPE_1
type: parsed
protocol: NECext
address: B8 00 00 00
command: 94 00 00 00
#
name: TAPE_2
type: parsed
protocol: NECext
address: B8 00 00 00
command: 95 00 00 00
#
name: VIDEO_1
type: parsed
protocol: NECext
address: B8 00 00 00
command: 96 00 00 00
#
name: TUNER_P.CALL_^
type: parsed
protocol: NECext
address: B8 00 00 00
command: 99 00 00 00
#
name: TUNER_UP
type: parsed
protocol: NECext
address: B8 00 00 00
command: 99 00 00 00
#
name: VOL_CONTROL_V
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9A 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9A 00 00 00
#
name: VOL_CONTROL_^
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9B 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9B 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9C 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9D 00 00 00
#
name: TUNER_DIRECT
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9E 00 00 00
#
name: DIRECT
type: parsed
protocol: NECext
address: B8 00 00 00
command: 9E 00 00 00
#
name: EQ.M.CALL
type: parsed
protocol: NECext
address: B8 00 00 00
command: C5 00 00 00
#
name: CD_STOP_[]
type: parsed
protocol: NECext
address: B8 00 00 00
command: C9 00 00 00
#
name: CD_PLAY/PAUSE_>/
type: parsed
protocol: NECext
address: B8 00 00 00
command: CB 00 00 00
#
name: CD_SKIP_<<
type: parsed
protocol: NECext
address: B8 00 00 00
command: CE 00 00 00
#
name: CD_SKIP_>>
type: parsed
protocol: NECext
address: B8 00 00 00
command: CF 00 00 00
#
name: TAPEA_REV_PLAY_<
type: parsed
protocol: NECext
address: B8 00 00 00
command: D0 00 00 00
#
name: TAPE_A_R_PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D0 00 00 00
#
name: TAPEA_PLAY_>
type: parsed
protocol: NECext
address: B8 00 00 00
command: D1 00 00 00
#
name: TAPE_A_PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D1 00 00 00
#
name: TAPEA_REW_<<
type: parsed
protocol: NECext
address: B8 00 00 00
command: D2 00 00 00
#
name: TAPE_A_REW
type: parsed
protocol: NECext
address: B8 00 00 00
command: D2 00 00 00
#
name: TAPEA_FF_>>
type: parsed
protocol: NECext
address: B8 00 00 00
command: D3 00 00 00
#
name: TAPE_A_FF
type: parsed
protocol: NECext
address: B8 00 00 00
command: D3 00 00 00
#
name: TAPEA_PAUSE_
type: parsed
protocol: NECext
address: B8 00 00 00
command: D4 00 00 00
#
name: TAPEA_STOP_[]
type: parsed
protocol: NECext
address: B8 00 00 00
command: D5 00 00 00
#
name: TAPE_A_STOP
type: parsed
protocol: NECext
address: B8 00 00 00
command: D5 00 00 00
#
name: TAPEA_REC
type: parsed
protocol: NECext
address: B8 00 00 00
command: D6 00 00 00
#
name: TAPE_A_REC
type: parsed
protocol: NECext
address: B8 00 00 00
command: D6 00 00 00
#
name: BYPASS
type: parsed
protocol: NECext
address: B8 00 00 00
command: D7 00 00 00
#
name: TAPEB_REV_PLAY_<
type: parsed
protocol: NECext
address: B8 00 00 00
command: D8 00 00 00
#
name: TAPE_B_R_PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D8 00 00 00
#
name: TAPEB_PLAY_>
type: parsed
protocol: NECext
address: B8 00 00 00
command: D9 00 00 00
#
name: TAPE_B_PLAY
type: parsed
protocol: NECext
address: B8 00 00 00
command: D9 00 00 00
#
name: TAPEB_REW_<<
type: parsed
protocol: NECext
address: B8 00 00 00
command: DA 00 00 00
#
name: TAPE_B_REW
type: parsed
protocol: NECext
address: B8 00 00 00
command: DA 00 00 00
#
name: TAPEB_FF_>>
type: parsed
protocol: NECext
address: B8 00 00 00
command: DB 00 00 00
#
name: TAPE_B_FF
type: parsed
protocol: NECext
address: B8 00 00 00
command: DB 00 00 00
#
name: TAPEB_PAUSE_
type: parsed
protocol: NECext
address: B8 00 00 00
command: DC 00 00 00
#
name: TAPEB_STOP_[]
type: parsed
protocol: NECext
address: B8 00 00 00
command: DD 00 00 00
#
name: TAPE_B_STOP
type: parsed
protocol: NECext
address: B8 00 00 00
command: DD 00 00 00
#
name: TAPEB_REC
type: parsed
protocol: NECext
address: B8 00 00 00
command: DE 00 00 00
#
name: TAPE_B_REC
type: parsed
protocol: NECext
address: B8 00 00 00
command: DE 00 00 00
