Filetype: IR signals file
Version: 1
#
name: CHANNELUP
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 00 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 02 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 03 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 05 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 06 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 07 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 09 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 0A 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 0B 00 00 00
#
name: erase
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 0C 00 00 00
#
name: tuneUp
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 0D 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 0F 00 00 00
#
name: decoder
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 14 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 16 00 00 00
#
name: AGAIN
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 18 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 19 00 00 00
#
name: store
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 1C 00 00 00
#
name: TuneDown
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 1D 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 1E 00 00 00
#
name: h/v
type: parsed
protocol: NECext
address: 42 FD 00 00
command: 1F 00 00 00
