Filetype: IR signals file
Version: 1
#
name: 0
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 00 00 00 00
command: 00 00 00 00
#
name: 1
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: ON_DEMAND
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: PPV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 01 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: PPV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 02 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: 00 00 00 00
command: 03 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: 00 00 00 00
command: 04 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: 00 00 00 00
command: 05 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: 00 00 00 00
command: 06 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: 00 00 00 00
command: 07 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: 00 00 00 00
command: 08 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 00 00 00 00
command: 09 00 00 00
#
name: CH+
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0B 00 00 00
#
name: CH_DN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 0C 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 10 00 00 00
#
name: OK/SELECT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: Unknown
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 00 00 00 00
command: 11 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 12 00 00 00
#
name: LAST
type: parsed
protocol: NECext
address: 00 00 00 00
command: 13 00 00 00
#
name: FAV
type: parsed
protocol: NECext
address: 00 00 00 00
command: 15 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 00 00 00 00
command: 19 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1B 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1C 00 00 00
#
name: FF
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1D 00 00 00
#
name: RW
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1E 00 00 00
#
name: PAUSE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 1F 00 00 00
#
name: GUIDE
type: parsed
protocol: NECext
address: 00 00 00 00
command: 30 00 00 00
#
name: RECORD
type: parsed
protocol: NECext
address: 00 00 00 00
command: 31 00 00 00
#
name: HELP[
type: parsed
protocol: NECext
address: 00 00 00 00
command: 32 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 34 00 00 00
#
name: DN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 35 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 36 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 00 00 00 00
command: 37 00 00 00
#
name: PLAY
type: parsed
protocol: NECext
address: 00 00 00 00
command: 38 00 00 00
#
name: STOP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 39 00 00 00
#
name: PAGE_UP
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3A 00 00 00
#
name: PAGE_DN
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3B 00 00 00
#
name: SKIP_30_SECONDS
type: parsed
protocol: NECext
address: 00 00 00 00
command: 3F 00 00 00
