Filetype: IR signals file
Version: 1
#
name: 1
type: parsed
protocol: NECext
address: B7 00 00 00
command: 00 00 00 00
#
name: 2
type: parsed
protocol: NECext
address: B7 00 00 00
command: 01 00 00 00
#
name: 3
type: parsed
protocol: NECext
address: B7 00 00 00
command: 02 00 00 00
#
name: 4
type: parsed
protocol: NECext
address: B7 00 00 00
command: 03 00 00 00
#
name: 5
type: parsed
protocol: NECext
address: B7 00 00 00
command: 04 00 00 00
#
name: 6
type: parsed
protocol: NECext
address: B7 00 00 00
command: 05 00 00 00
#
name: 7
type: parsed
protocol: NECext
address: B7 00 00 00
command: 06 00 00 00
#
name: 8
type: parsed
protocol: NECext
address: B7 00 00 00
command: 07 00 00 00
#
name: 9
type: parsed
protocol: NECext
address: B7 00 00 00
command: 08 00 00 00
#
name: 0
type: parsed
protocol: NECext
address: B7 00 00 00
command: 09 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: B7 00 00 00
command: 0B 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: B7 00 00 00
command: 10 00 00 00
#
name: CHANNELUP
type: parsed
protocol: NECext
address: B7 00 00 00
command: 10 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: B7 00 00 00
command: 11 00 00 00
#
name: CHANNELDOWN
type: parsed
protocol: NECext
address: B7 00 00 00
command: 11 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: B7 00 00 00
command: 12 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: B7 00 00 00
command: 12 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: B7 00 00 00
command: 13 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: B7 00 00 00
command: 13 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: B7 00 00 00
command: 14 00 00 00
#
name: DSS_POWER
type: parsed
protocol: NECext
address: B7 00 00 00
command: 15 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: B7 00 00 00
command: 15 00 00 00
#
name: TV/VIDEO
type: parsed
protocol: NECext
address: B7 00 00 00
command: 25 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: B7 00 00 00
command: 2E 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: B7 00 00 00
command: 2F 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: B7 00 00 00
command: 38 00 00 00
#
name: DISPLAY
type: parsed
protocol: NECext
address: B7 00 00 00
command: 3A 00 00 00
#
name: JUMP
type: parsed
protocol: NECext
address: B7 00 00 00
command: 3B 00 00 00
#
name: INDEX
type: parsed
protocol: NECext
address: B7 00 00 00
command: 3F 00 00 00
#
name: CATEGORY
type: parsed
protocol: NECext
address: B7 00 00 00
command: 44 00 00 00
#
name: AUDIO
type: parsed
protocol: NECext
address: B7 00 00 00
command: 47 00 00 00
#
name: CABLE
type: parsed
protocol: NECext
address: B7 00 00 00
command: 4E 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: B7 00 00 00
command: 60 00 00 00
#
name: VIDEO
type: parsed
protocol: NECext
address: B7 00 00 00
command: 61 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: B7 00 00 00
command: 63 00 00 00
#
name: TV/DSS
type: parsed
protocol: NECext
address: B7 00 00 00
command: 69 00 00 00
#
name: JUMP
type: parsed
protocol: NECext
address: B7 00 00 00
command: 6C 00 00 00
#
name: INFO
type: parsed
protocol: NECext
address: B7 00 00 00
command: 6E 00 00 00
#
name: FAVORITES
type: parsed
protocol: NECext
address: B7 00 00 00
command: 6F 00 00 00
#
name: UP_ARROW
type: parsed
protocol: NECext
address: B7 00 00 00
command: 72 00 00 00
#
name: DOWN_ARROW
type: parsed
protocol: NECext
address: B7 00 00 00
command: 73 00 00 00
#
name: RIGHT_ARROW
type: parsed
protocol: NECext
address: B7 00 00 00
command: 74 00 00 00
#
name: LEFT_ARROW
type: parsed
protocol: NECext
address: B7 00 00 00
command: 75 00 00 00
#
name: SELECT
type: parsed
protocol: NECext
address: B7 00 00 00
command: 76 00 00 00
