Filetype: IR signals file
Version: 1
# 
name: Power
type: parsed
protocol: NECext
address: D2 03 00 00
command: 04 FB 00 00
# 
name: Standby
type: parsed
protocol: NECext
address: D2 04 00 00
command: 47 B8 00 00
# 
name: Vol_up
type: parsed
protocol: NECext
address: D2 03 00 00
command: 02 FD 00 00
# 
name: Vol_dn
type: parsed
protocol: NECext
address: D2 03 00 00
command: 03 FC 00 00
# 
name: InputUp
type: parsed
protocol: NECext
address: D2 04 00 00
command: 1E E1 00 00
# 
name: InputDown
type: parsed
protocol: NECext
address: D2 04 00 00
command: 1F E0 00 00
# 
name: Muting
type: parsed
protocol: NECext
address: D2 03 00 00
command: 05 FA 00 00
# 
name: Dimmer
type: parsed
protocol: NECext
address: D2 03 00 00
command: 95 6A 00 00
# 
name: Display
type: parsed
protocol: NECext
address: D2 04 00 00
command: 55 AA 00 00
# 
name: Play
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1B E4 00 00
# 
name: Pause
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1F E0 00 00
# 
name: Stop
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1C E3 00 00
# 
name: Rewind
type: parsed
protocol: NECext
address: D2 03 00 00
command: 8B 74 00 00
# 
name: FF
type: parsed
protocol: NECext
address: D2 03 00 00
command: 8A 75 00 00
# 
name: Back
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1E E1 00 00
# 
name: Forward
type: parsed
protocol: NECext
address: D2 03 00 00
command: 1D E2 00 00
# 
name: Random
type: parsed
protocol: NECext
address: D2 04 00 00
command: 57 A8 00 00
# 
name: Repeat
type: parsed
protocol: NECext
address: D2 04 00 00
command: 56 A9 00 00
# 
name: Scroll
type: parsed
protocol: NECext
address: D2 04 00 00
command: 12 ED 00 00
# 
name: PlaylistUp
type: parsed
protocol: NECext
address: D2 09 00 00
command: 52 AD 00 00
# 
name: PlaylistDn
type: parsed
protocol: NECext
address: D2 09 00 00
command: 53 AC 00 00
# 
name: AlbumUp
type: parsed
protocol: NECext
address: D2 09 00 00
command: 50 AF 00 00
# 
name: AlbumDn
type: parsed
protocol: NECext
address: D2 09 00 00
command: 51 AE 00 00
# 
name: Band
type: parsed
protocol: NECext
address: D2 04 00 00
command: 8A 75 00 00
# 
name: FMMode
type: parsed
protocol: NECext
address: D2 09 00 00
command: D3 2C 00 00
# 
name: PresetUp
type: parsed
protocol: NECext
address: D2 03 00 00
command: 00 FF 00 00
# 
name: PresetDn
type: parsed
protocol: NECext
address: D2 03 00 00
command: 01 FE 00 00
# 
name: TuningUp
type: parsed
protocol: NECext
address: D2 09 00 00
command: 40 BF 00 00
# 
name: TuningDn
type: parsed
protocol: NECext
address: D2 09 00 00
command: 41 BE 00 00
# 
name: PlayMode
type: parsed
protocol: NECext
address: D2 04 00 00
command: 08 F7 00 00
# 
name: GroupSearch
type: parsed
protocol: NECext
address: D2 04 00 00
command: 81 7E 00 00
# 
name: Memory
type: parsed
protocol: NECext
address: D2 03 00 00
command: 49 B6 00 00
# 
name: Enter
type: parsed
protocol: NECext
address: D2 04 00 00
command: 46 B9 00 00
# 
name: 1
type: parsed
protocol: NECext
address: D2 03 00 00
command: D5 2A 00 00
# 
name: 2
type: parsed
protocol: NECext
address: D2 03 00 00
command: D6 29 00 00
# 
name: 3
type: parsed
protocol: NECext
address: D2 03 00 00
command: D7 28 00 00
# 
name: 4
type: parsed
protocol: NECext
address: D2 03 00 00
command: D8 27 00 00
# 
name: 5
type: parsed
protocol: NECext
address: D2 03 00 00
command: D9 26 00 00
# 
name: 6
type: parsed
protocol: NECext
address: D2 03 00 00
command: DA 25 00 00
# 
name: 7
type: parsed
protocol: NECext
address: D2 03 00 00
command: DB 24 00 00
# 
name: 8
type: parsed
protocol: NECext
address: D2 03 00 00
command: DC 23 00 00
# 
name: 9
type: parsed
protocol: NECext
address: D2 03 00 00
command: DD 22 00 00
# 
name: GT10
type: parsed
protocol: NECext
address: D2 03 00 00
command: DF 20 00 00
# 
name: 10_0
type: parsed
protocol: NECext
address: D2 03 00 00
command: DE 21 00 00
# 
name: CLR
type: parsed
protocol: NECext
address: D2 03 00 00
command: 9E 61 00 00
