Filetype: IR signals file
Version: 1
# 
# LG Remote AKB72915206
#
# Captured by: emptythevoid
#
name: Power
type: parsed
protocol: NEC
address: 04 00 00 00
command: 08 00 00 00
# 
name: Energy_saving
type: parsed
protocol: NEC
address: 04 00 00 00
command: 95 00 00 00
# 
name: Av_mode
type: parsed
protocol: NEC
address: 04 00 00 00
command: 30 00 00 00
# 
name: Input
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0B 00 00 00
# 
name: Tv
type: parsed
protocol: NEC
address: 04 00 00 00
command: 0F 00 00 00
# 
name: 1
type: parsed
protocol: NEC
address: 04 00 00 00
command: 11 00 00 00
# 
name: 2
type: parsed
protocol: NEC
address: 04 00 00 00
command: 12 00 00 00
# 
name: 3
type: parsed
protocol: NEC
address: 04 00 00 00
command: 13 00 00 00
# 
name: 4
type: parsed
protocol: NEC
address: 04 00 00 00
command: 14 00 00 00
# 
name: 5
type: parsed
protocol: NEC
address: 04 00 00 00
command: 15 00 00 00
# 
name: 6
type: parsed
protocol: NEC
address: 04 00 00 00
command: 16 00 00 00
# 
name: 7
type: parsed
protocol: NEC
address: 04 00 00 00
command: 17 00 00 00
# 
name: 8
type: parsed
protocol: NEC
address: 04 00 00 00
command: 18 00 00 00
# 
name: 9
type: parsed
protocol: NEC
address: 04 00 00 00
command: 19 00 00 00
# 
name: 0
type: parsed
protocol: NEC
address: 04 00 00 00
command: 10 00 00 00
# 
name: -
type: parsed
protocol: NEC
address: 04 00 00 00
command: 4C 00 00 00
# 
name: Flashbk
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1A 00 00 00
# 
name: Vol_up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 02 00 00 00
# 
name: Vol_dn
type: parsed
protocol: NEC
address: 04 00 00 00
command: 03 00 00 00
# 
name: Ch_next
type: parsed
protocol: NEC
address: 04 00 00 00
command: 00 00 00 00
# 
name: Ch_prev
type: parsed
protocol: NEC
address: 04 00 00 00
command: 01 00 00 00
# 
name: Fav
type: parsed
protocol: NEC
address: 04 00 00 00
command: 1E 00 00 00
# 
name: Ratio
type: parsed
protocol: NEC
address: 04 00 00 00
command: 79 00 00 00
# 
name: Mute
type: parsed
protocol: NEC
address: 04 00 00 00
command: 09 00 00 00
# 
name: Menu
type: parsed
protocol: NEC
address: 04 00 00 00
command: 43 00 00 00
# 
name: Info
type: parsed
protocol: NEC
address: 04 00 00 00
command: AA 00 00 00
# 
name: Q_menu
type: parsed
protocol: NEC
address: 04 00 00 00
command: 45 00 00 00
# 
name: Up
type: parsed
protocol: NEC
address: 04 00 00 00
command: 40 00 00 00
# 
name: Left
type: parsed
protocol: NEC
address: 04 00 00 00
command: 07 00 00 00
# 
name: Right
type: parsed
protocol: NEC
address: 04 00 00 00
command: 06 00 00 00
# 
name: Down
type: parsed
protocol: NEC
address: 04 00 00 00
command: 41 00 00 00
# 
name: Enter
type: parsed
protocol: NEC
address: 04 00 00 00
command: 44 00 00 00
# 
name: Back
type: parsed
protocol: NEC
address: 04 00 00 00
command: 28 00 00 00
# 
name: Simplink
type: parsed
protocol: NEC
address: 04 00 00 00
command: 7E 00 00 00
# 
name: Exit
type: parsed
protocol: NEC
address: 04 00 00 00
command: 5B 00 00 00
# 
name: Red
type: parsed
protocol: NEC
address: 04 00 00 00
command: 72 00 00 00
# 
name: Green
type: parsed
protocol: NEC
address: 04 00 00 00
command: 71 00 00 00
# 
name: Yellow
type: parsed
protocol: NEC
address: 04 00 00 00
command: 63 00 00 00
# 
name: Blue
type: parsed
protocol: NEC
address: 04 00 00 00
command: 61 00 00 00
# 
name: Stop
type: parsed
protocol: NEC
address: 04 00 00 00
command: B1 00 00 00
# 
name: Play
type: parsed
protocol: NEC
address: 04 00 00 00
command: B0 00 00 00
# 
name: Pause
type: parsed
protocol: NEC
address: 04 00 00 00
command: BA 00 00 00
# 
name: Rew
type: parsed
protocol: NEC
address: 04 00 00 00
command: 8F 00 00 00
# 
name: Fwd
type: parsed
protocol: NEC
address: 04 00 00 00
command: 8E 00 00 00
