Filetype: IR signals file
Version: 1
#
name: POWER
type: parsed
protocol: NECext
address: 01 00 00 00
command: 00 00 00 00
#
name: MUTE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 01 00 00 00
#
name: +/-5dB
type: parsed
protocol: NECext
address: 01 00 00 00
command: 02 00 00 00
#
name: NORMAL
type: parsed
protocol: NECext
address: 01 00 00 00
command: 03 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 01 00 00 00
command: 04 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 01 00 00 00
command: 05 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 06 00 00 00
#
name: SUBTITLE
type: parsed
protocol: NECext
address: 01 00 00 00
command: 07 00 00 00
#
name: CENTER_-
type: parsed
protocol: NECext
address: 01 00 00 00
command: 08 00 00 00
#
name: CENTER_+
type: parsed
protocol: NECext
address: 01 00 00 00
command: 09 00 00 00
#
name: SURROUND_-
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0A 00 00 00
#
name: SURROUND_+
type: parsed
protocol: NECext
address: 01 00 00 00
command: 0B 00 00 00
