Filetype: IR signals file
Version: 1
#
name: VIDEO
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 03 00 00 00
#
name: computer_1
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 04 00 00 00
#
name: computer_2
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 05 00 00 00
#
name: auto_adj
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 06 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 08 00 00 00
#
name: picture
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 0D 00 00 00
#
name: aspect
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 10 00 00 00
#
name: POWER
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 14 00 00 00
#
name: ENTER
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 17 00 00 00
#
name: EXIT
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 25 00 00 00
#
name: PAGEUP
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 2A 00 00 00
#
name: PAGEDOWN
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 2B 00 00 00
#
name: l_click
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 2C 00 00 00
#
name: r_click
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 2D 00 00 00
#
name: MENU
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 46 00 00 00
#
name: pic-MUTE
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 47 00 00 00
#
name: VOL+
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 48 00 00 00
#
name: VOL-
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 49 00 00 00
#
name: freeze
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 4C 00 00 00
#
name: HELP
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 4E 00 00 00
#
name: magnify_plus
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 89 00 00 00
#
name: magnify_minus
type: parsed
protocol: NECext
address: 18 E9 00 00
command: 8A 00 00 00
#
name: UP
type: parsed
protocol: NECext
address: 18 E9 00 00
command: B8 00 00 00
#
name: RIGHT
type: parsed
protocol: NECext
address: 18 E9 00 00
command: BA 00 00 00
#
name: DOWN
type: parsed
protocol: NECext
address: 18 E9 00 00
command: BC 00 00 00
#
name: LEFT
type: parsed
protocol: NECext
address: 18 E9 00 00
command: BE 00 00 00
#
name: s-video
type: parsed
protocol: NECext
address: 18 E9 00 00
command: C6 00 00 00
